[image: image1.jpg]



FIG. 1-8
LIFTING CYLINDER HEAD ASSEMBLY

13. Apply lifting eye bolts in tapped holes to the right and left of the nozzle hole and lift cylinder head slowly and carefully with cylinder head lifting assembly, Fig. 1-8, using hoist attached to overhead support. Cover air, exhaust and cylinder openings to prevent any foreign matter from entering. 

NOTE: In removing a cylinder head from a Freight-Passenger locomotive engine an overhead support integral with the roof is provided to which a hoist maybe attached to facilitate the removal of the cylinder head. On the Road Switcher the cylinder heads may be removed through the hood roof hatches with a hoist or an overhead crane. 
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